Information and data storage lab 1

Lab questions

1. Model VNXe3200
2. Software version 3.0.0.2585212
3. 10.3 TB
4. 1.0 TB
5. 307.1 GB
6. Alerts are dispatched for things such as when the normal operation of a device is ensured or when processes have stopped.
7. None listed
8. 4 FC ports
9. NFS and CIFS are both on the system
10. There are 2 LUNS using FC that are not configured. There are 4 LUNS using ISCSI that are configured and labeled 0-4
11. The storage pool is comprised of 2 RAID 5’s with 3.2TB in performance disks and 7.1TB in storage disks
12. Yes the pool supports FAST VP
13. All disks are a part of the pool but not all disks are filled, so there are some “spares”
14. Under the hosts tab the options “Create host”, “Create Subnet”, and “Create netgroup” all become available for use
15. There are 4 hosts available. 10.244.214.22 is an automatically created host using vmware esxi 5.0.
16. Dwa
17. Dwa
18. Dwa
19. Dwa